**HYDRAULIC JACK**

**ADDING OIL**

**RED TRANSMITTION FLUID – ATF**

JACKS ARE ***ON*** CAMPER:

Retract jacks all the way IN

Remove **fill hole Hex Head Bolt**

Use Syringe to fill up to the bottom of the fill hole

JACKS ARE ***OFF*** CAMPER:

Lay jacks on side.

Pour ATF fluid into fill hole.

Do not replace hex bolt.

Stand up jack to let excess oil to drain out.

Replace Hex Bolt.